IEEE P802.22
Wireless RANs

|  |
| --- |
| Proposed Resolution to CID 35  |
| Date: 2014-09-18 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Shigenobu　 Sasaki | Niigata University | 8050 Ikarashi 2-no-cho, Niigata, 950-2181 Japan | 81-25-262-6737 | shinsasaki@ieee.org |
| Takuto Uchida | Niigata University | 8050 Ikarashi 2-no-cho, Niigata, 950-2181 Japan | 81-25-262-6737 | u-takuto@telecom0. eng.niigata-u.ac.jp |

Abstract

This document presents a proposed resolution to Comment ID 35 on the coded 256QAM and multidimentional trellis coded modulation (MD-TCM) in LB commetns for IEEE Draft Std. 802.22b D2.0. The content of this document is potentially included into the updated version of the IEEE 802.22b draft standard.

**Notice:** This document has been prepared to assist IEEE 802.22. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.22.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures

<[**http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf**](http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair Apurva Mody <apurva.mody@ieee.org> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.22 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <****patcom@ieee.org****>**.

1. Introduction

This contribution provides the proposed resolution for the following comments in LB2 for the IEEE Draft Std. 802.22b D2.0 [1]. Additional changes are also proposed associated with this comment resolution.

|  |  |  |  |
| --- | --- | --- | --- |
| **ID** | **Commenter Name** | **Comment** | **Suggested Remedy** |
| 35 | Shigenobu Sasaki | Table 228: Fill all the TBDs in the table.  | Fill all the TBDs in the table. |

1. Proposed resolution

 *[Start of proposed changes.]*

***Change Table 228 as indicated.***

Table 228 — Normalized CNR per modulation for BER= 2\*10-4

|  |  |
| --- | --- |
| **Modulation - FEC rate** | **Normalized CNR (dB)** |
| **AWGN****(default)** | **Multipath Channel**8F**[[1]](#footnote-1)** *(informative)* |
| CDMA code | 1.2 | 5 |
| QPSK, rate: 1/2 | 4.3 | 8.1 |
| QPSK, rate: 2/3 | 6.1 | 11.6 |
| QPSK, rate: 3/4 | 7.1 | 14.0 |
| QPSK, rate: 5/6 | 8.1 | 17.8 |
| 16-QAM, rate: 1/2 | 10.2 | 14.8 |
| 16-QAM, rate: 2/3 | 12.4 | 20.3 |
| 16-QAM, rate: 3/4 | 13.5 | 24.6 |
| 16-QAM, rate: 5/6 | 14.8 | 28.6 |
| 64-QAM, rate: 1/2 | 15.6 | 20.5 |
| 64-QAM, rate: 2/3 | 18.3 | 26.2 |
| 64-QAM, rate: 3/4 | 19.7 | 31.8 |
| 64-QAM, rate: 5/6 | 20.9 | 40.4 |
| 256-QAM, rate: 1/2 | 21.5 | 25.7 |
| 256-QAM, rate: 2/3 | 25.0 | 30.0 |
| 256-QAM, rate: 3/4 | 27.2 | 32.6 |
| 256-QAM, rate: 5/6 | 29.0 | 36.1 |
| 256-QAM, rate: 7/8 | 31.2 | 39.8 |
| 4D-TCM 48QAM | 19.4 | 26.8 |
| 4D-TCM 192 QAM | 27.5 | 32.5 |

*[End of proposed change]*

1. Additional Proposed Changes

The following text changes are proposed associated with the changes in the previous section:

*[Start of proposed changes.]*

***Change the text in the IEEE 802.22-2011[2] as indicated.***

**(Page 356, below Equation (13))**

This resulting value Pnew is updated based on the value Prange transmitted regularly to the CPE by the BS through the RNG-CMD MAC message (see 7.7.6) to keep the TPC of the RF link up-to-date. The CPE shall be calibrated by the manufacturer so that the actual EIRP density per subcarrier transmitted by the CPE corresponds to the level indicated by the Prange variable resulting from the RNG-CMD message (within 0.5 dB). The default normalized CNR values per modulation for the binary convolutional code (BCC) and multidimensional trellis coded modulation (MD-TCM), except for the CDMA code, are given in Table228. These values may be overridden by the BS by using a dedicated UCD message (see Table33). The second column is the default value and third column is informative and indicative of the modulation performance in a multipath channel.

*[End of proposed change]*

**References:**

1. IEEE Draft Std. 802.22b D2.0, 2014
2. IEEE Std. 802.22-2011, July 2011
1. The multipath channel used for the calculations is defined on 6 paths as follows: excess delay: -3, 0, 2, 4, 7 and 11 μsec; relative amplitude: -6, 0, -7, -22, -16 and -20 dB; the phase for each path is random. The delay, amplitude and phase are assumed to be constant over the period of one symbol. [↑](#footnote-ref-1)