IEEE P802.22 Wireless RANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Errata – 802.22 base std, LTS and STS | | | | |
| Date: 2016-03-15 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Ivan Reede | AmeriSys | Montreal, Quebec, Canada | 514-620-8522 | i\_reede@amerisys.com |
| Gerald Chouinard | AmeriSys | Gatineau, Quebec, Canada | 514-620-8522 | [gerald@amerisys.com](mailto:apurva_mody@yahoo.com) |

**Notice:** This document has been prepared to assist IEEE 802.22. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.22.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures

<[**http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf**](http://standards.ieee.org/guides/bylaws/sb-bylaws.pdf)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair Apurva N. Mody <[**apurva.mody@ieee.org**](mailto:apurva.mody@ieee.org)> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.22 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <**[**patcom@ieee.org**](mailto:patcom@ieee.org)**>**.

Abstract

In our work to create test vectors and testing an implementation for compliance to the base 802.22 standard, it was discovered that the intended operation of normalization is broken by an erroneous mathematical expression describing both the STS and LTS.

Also, the lower and upper halves of the spectrum are inverted (confirmed on the spectrum analyser) in a mathematical expression describing the LTS due to an erroneous swap of indices 115 and 536.

***Proposed corrections to sub-clauses 9.4.1.1.1 and 9.4.1.1.2  
 of the IEEE Std 802.22TM- 2011***

Generation of STS

[Change all occurrences of the normalization factor SQRT(NT/420) for SQRT(1680/NT)

Generation of LTS

First, a periodic sequence with a period of 1024 is generated using a pseudo-noise (PN) sequence generator with a polynomial of. 1275HFigure 1 depicts an implementation of this PN sequence generator using a Linear Feedback Shift Register.



1. — Structure of a Linear Feedback Shift Register implementation  
   for the given LTS polynomial

The LTS sequence generator is initialized to a value of 11 1111 1111. The resultant  sequence of 1023 samples (using BPSK mapping) is given as follows:

 = {1, 1, 1, 1, 1, 1, 1, 1, 1, 1, –1, –1, 1, 1, 1, –1, 1, –1, 1, 1, … , 1, –1, 1, 1, –1, –1, –1, 1, –1, –1, –1, –1, 1, 1, –1, 1, –1, –1, 1, –1}

Second, define and respectively. The first 420 binary values of these sequences are as follows:

S115(0:419) = {1, –1, 1, –1, 1, –1, –1, –1, –1, 1, 1, 1, –1, 1, 1, 1, 1, 1, 1, 1, …, 1, 1, –1, 1, –1, 1, 1, 1, –1, 1, 1, –1, –1, 1, –1, –1, 1, 1, 1, 1}, and

S536(0:419) = {1, 1, 1, 1, –1, –1, –1, 1, 1, 1, –1, –1, –1, 1, –1, –1, –1, 1, 1, –1, …, 1, –1, –1, 1, –1, –1, 1, 1, 1, –1, –1, –1, 1, 1, –1, 1, 1, 1, 1, 1}, and

For illustration only, consider that after resetting the LTS generator, the pair of sequences { S115, S536,} can be represented in Hexadecimal format where the elements with amplitude value of –1 are mapped to bit0 (bit zero) and the elements with value of +1 are mapped to bit1 (bit one). These sequences can therefore be represented in hex format (bit ordering from left to right) as follows:

{S115hex}= A877F40C94889D20B91E7FB49616CB714A17845A62EE00A795947CC27EFBBD3E32F5B7E0FE2607056F6669D872C8A0376E8ED764F

{S536hex}= F1C4677539900F45F5E42A3418663A12B8F6C1081350487D8D55D344BACF02CD9C9BCD68C4932A67D2AC0473878B1F970A2A938DF

The coefficients of the 2048 frequency elements to be presented at the input of the inverse DFT are then formed from the above two sequences using the following equation where *NT* represents the number of used subcarriers:

[ Swap indices 536 and 115.] (3)

and results in the long training (LT) sequence as shown below:

PLT (–1024:–841) = {0, 0, 0, 0, 0, …, 0, 0, 0, 0, 0}

PLT (–840:–1) =  {1, 0, –1, 0, 1, 0, –1, 0, 1, 0, –1, 0, –1, 0, –1, 0, –1, 0, 1, 0, …, 1, 0, –1, 0, –1, 0, 1, 0, –1, 0, –1, 0, 1, 0, 1, 0, 1, 0, 1, 0}

PLT(0) = 0

PLT(1:840) =  {0, 1, 0, 1, 0, 1, 0, 1, 0, –1, 0, –1, 0, –1, 0, 1, 0, 1, 0, …, 0, –1, 0, –1, 0, 1, 0, 1, 0, –1, 0, 1, 0, 1, 0, 1, 0, 1, 0, 1}

PLT (841:1023) = {0, 0, 0, 0, 0, …, 0, 0, 0, 0, 0}

Taking the inverse DFT of PLT will result in 2 repetitions of a 1024-sample vector in the time domain. The factor  is used to normalize the signal energy, where *NT* represents the number of used subcarriers.

[Change all occurrences of the normalization factor SQRT(NT/840) for SQRT(1680/NT)