|  |
| --- |
| IEEE 802 Standards for Smart Grid |
|  |  |
|  |
|  | **IEEE P802.24****Smart Grid Technical Advisory Group**  |
|  |  |



**Trademarks and Disclaimers**

*IEEE believes the information in this publication is accurate as of its publication date; such information is subject to change without notice. IEEE is not responsible for any inadvertent errors.*

*The Institute of Electrical and Electronics Engineers, Inc.*

*3 Park Avenue, New York, NY 10016-5997, USA*

*Copyright © 2024 by The Institute of Electrical and Electronics Engineers, Inc.
All rights reserved. Published Month 20xx. Printed in the United States of America.*

*IEEE is a registered trademark in the U. S. Patent & Trademark Office, owned by The Institute of Electrical and Electronics Engineers, Incorporated.*

PDF: ISBN 978-0-7381-xxxx-x STDVxxxxx

Print: ISBN 978-0-7381-xxxx-x STDPDVxxxxx

*IEEE prohibits discrimination, harassment, and bullying. For more information, visit* [*http://www.ieee.org/web/aboutus/whatis/policies/p9-26.html*](http://www.ieee.org/web/aboutus/whatis/policies/p9-26.html)*.*

*No part of this publication may be reproduced in any form, in an electronic retrieval system, or otherwise, without the prior written permission of the publisher.*

*To order IEEE Press Publications, call 1-800-678-IEEE.*

*Find IEEE standards and standards-related product listings at:* [*http://standards.ieee.org*](http://standards.ieee.org)

**Notice and Disclaimer of Liability
Concerning the Use of IEEE-SA Documents**

*This IEEE Standards Association (“IEEE-SA”) publication (“Work”) is not a consensus standard document. Specifically, this document is NOT AN IEEE STANDARD. Information contained in this Work has been created by, or obtained from, sources believed to be reliable, and reviewed by members of the IEEE P802.24 Smart Grid Technical Advisory Group that produced this Work. IEEE and the* *IEEE P802.24 Smart Grid Technical Advisory Group members expressly disclaim all warranties (express, implied, and statutory) related to this Work, including, but not limited to, the warranties of: merchantability; fitness for a particular purpose; non-infringement; quality, accuracy, effectiveness, currency, or completeness of the Work or content within the Work. In addition, IEEE and the IEEE P802.24 Smart Grid Technical Advisory Group members disclaim any and all conditions relating to: results; and workmanlike effort. This IEEE P802.24 Smart Grid Technical Advisory Group document is supplied “AS IS” and “WITH ALL FAULTS.”*

*Although the IEEE P802.24 Smart Grid Technical Advisory Group members who have created this Work believe that the information and guidance given in this Work serve as an enhancement to users, all persons must rely upon their own skill and judgment when making use of it. IN NO EVENT SHALL IEEE OR IEEE P802.24 SMART GRID TECHNICAL ADVISORY GROUP MEMBERS BE LIABLE FOR ANY ERRORS OR OMISSIONS OR DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO: PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS WORK, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE AND REGARDLESS OF WHETHER SUCH DAMAGE WAS FORESEEABLE*.

*Further, information contained in this Work may be protected by intellectual property rights held by third parties or organizations, and the use of this information may require the user to negotiate with any such rights holders in order to legally acquire the rights to do so. IEEE and the IEEE P802.24 Smart Grid Technical Advisory Group members make no assurances that the use of the material contained in this work is free from patent infringement.* [*Essential Patent Claims*](http://standards.ieee.org/develop/policies/bylaws/sect6-7.html#essential-patent-claim) *may exist for which no assurances have been made to the IEEE, whether by participants in this IEEE P802.24 Smart Grid Technical Advisory Group activity or entities outside the activity. The IEEE is not responsible for identifying essential patent claims for which a license may be required, for conducting inquiries into the legal validity or scope of* [*patents claims*](http://standards.ieee.org/develop/policies/bylaws/sect6-7.html#patent-claim)*, or determining whether any licensing terms or conditions, if any, or any licensing agreements are reasonable or non-discriminatory. Users are expressly advised that determination of the validity of any patent rights, and the risk of infringement of such rights, is entirely their own responsibility. No commitment to grant licenses under patent rights on a reasonable or non-discriminatory basis has been sought or received from any rights holder. The policies and procedures under which this document was created can be viewed at* [*http://standards.ieee.org/about/sasb/iccom/*](http://standards.ieee.org/about/sasb/iccom/)*.*

*This Work is published with the understanding that IEEE and the IEEE P802.24 Smart Grid Technical Advisory Group members are supplying information through this Work, not attempting to render engineering or other professional services. If such services are required, the assistance of an appropriate professional should be sought. IEEE is not responsible for the statements and opinions advanced in this Work.*

Contents

## INTRODUCTION 1

## History and values of IEEE 802 1

## Characteristics of IEEE 802 networks that support Smart Grid applications 2

## APPLICATIONS FOR SMART GRID 3

## AMI 3

## DA 3

## Application requirements for network communications 3

## Security 3

## Non-mains powered operations (for some devices) 4

## Coverage requirements 4

## Advantages of IEEE 802 networks 4

## CONCLUSIONS 5

## REFERENCES 6

IEEE 802 Standards for Smart Grid

## Introduction to the 2024 revision

This white paper was first published in 2014. Over the past decade, the utility industry has seen many changes, and IEEE 802 has continued to release new standards and revisions. The term “Smart Grid” is less frequently used now, because it became associated with specific use cases, such as metering. Terms such as “Grid Modernization” and “Integration of Renewables” better express the system-level changes that are driving an increasing requirement and dependence on telecommunications to enable the operation of the future grid. The title will remain unchanged for historical continuity.

The use of communication in the grid is a type IoT, in the sense that the communication is primarily machine to machine over a collection of multiple IP-based networks. It diverges from typical IoT because the networks that are used for utility grids are typically not carried over the public Internet, but are private and secured.

## History and values of IEEE 802

IEEE 802® is the leading standards development organization for networking. IEEE 802 is actively developing standards for both wired and wireless networks.

Smart Grid is defined as an evolution of the energy supply and consumption infrastructure that will enable providers and consumers with unprecedented levels of reliability and control while reducing the adverse environmental impact of energy generation and consumption. One of the key aspects of the Smart Grid is the underlying communication between the various network elements.

 The first IEEE 802 network standard, IEEE Std 802.3™ (Ethernet), was approved more than 40 years ago. The first IEEE 802 wireless standard, IEEE Std 802.11™, was approved in 1997, and has evolved through seven generations of increasing performance. IEEE Std 802.15™ and IEEE Std 802.16™ were both initiated in 1999 and have achieved substantial success as well. The IEEE 802.15 SUN PHY has launched the Wi-SUN Alliance specifically targeting utility use cases. While IEEE 802.16 was unsuccessful in the commercial cellular market, the standard’s narrow channel amendments 802.16s and 802.16t provide options for operation in licensed spectrum with channels too small to support LTE. Other groups in IEEE 802 that are relevant to Smart Grid applications are as follows:

* IEEE Std 802.1™ provides foundational bridging, time-sensitive networks, and security capabilities. 802.1 standards are often referred to by other standards.
* IEEE Std 802.21d developed a multicast group management amendment that was seen as promising for use in electrical metering networks. 802.21 has entered into hibernation, 802.21d did not achieve market adoption.
* IEEE Std 802.22™ for wireless regional area networks (WRAN) in the TV white space (TVWS) bands was a promising technology for Smart Grid when introduced. The use of unused channels for long-range outdoor communication was well suited to many smart grid use cases. The FCC auctioned 600 MHz spectrum in 2017 for cellular use, resulting in the elimination of unused TV channels, except in the most remote locations. 802.22 has entered into hibernation.

Placeholder for section on the introduction of spectrum sharing approaches in the 2014-2024 decade.

IEEE 802 has endorsed the OpenStand principles (see [http://open-stand.org/](http://open-stand.org/%20)), which include cooperation, adherence to principles, collective empowerment, availability, and voluntary adoption. These principles are part of the process IEEE 802 uses to create high-quality, widely-adopted standards.

Many utility applications are examples of the broader application area of Machine-to-machine (M2M) technology, which enables devices to communicate with each other. There are three general layers in M2M, as shown in Figure 1.

 

Figure 1: Layering of M2M technology

The application layer, which is the highest layer, provides the relevant application data. Organizations such as the Smart Grid Interoperability Panel (SGIP) and IEC, and other IEEE projects (Such as IEEE 1547 and IEEE 2030) are involved in the definition of this layer.

A middle layer called the common service layer enables the exchange of information between the application layer and the access independent underlying network. Organizations such as oneM2M are leading the effort to standardize this layer.

Below the common service layer is the underlying network layer. IEEE 802 standards provide underlying networks with enhanced coverage and accessibility, quality of service, security (such as authentication and encryption), and reliability (high availability of network infrastructure). IEEE 802 standards can also provide additional capabilities for an ad-hoc self-organizing network, such as low cost, low power, low duty cycle, and low data rate.

Some IEEE 802 networking technologies offer the ability to bound communication latency of a link. IEEE 802 technologies that are not based on multi-hop networks will generally offer better ability to bound communication latency.

A list of Smart Grid standards that focus on PHY and MAC layer have been documented and approved by IEEE 802 [1].

## Characteristics of IEEE 802 networks that support Smart Grid applications

IEEE 802 networking technologies bring the following advantages to Smart Grid communications:

* Enterprise grade security compatibility
* Huge ecosystem (billions of products, hundreds of manufacturers)
* Long-term (20 year), battery-powered operation
* Continued operation during line fault events when using wireless media
* Wide choice of products across the spectrum of power versus performance
* Ability to be implemented in resource-constrained devices
* Ongoing development of standards to address changing environment and technology
* Wireless standards that operate in a licensed and license-exempt spectrum
* Offers a rich set of data rate/range/latency tradeoffs
* Common upper layer interface to seamlessly integrate into existing IT systems

Utilities have historically owned licensed spectrum, but the allocations are typically a group of narrow-band channels intended for Land Mobile Radio voice operation. As Smart Grid use cases demand additional bandwidth, additional spectrum was needed. Operation in license-exempt spectrum offers an alternative for utilities, but also introduces new constraints from limited power and greater interference. Shared spectrum has also been explored by utilities. TV White Space (TVWS) is an example a first step towards spectrum sharing between licensed and license exempt services, but was limited by the auctioning of most of the TV spectrum. Citizens Broadband Radio Service (CBRS) defines shared operation in the 3.65 GHz band and has been adopted by many utilities.

Multi-hop mesh networks are built on the MAC/PHY of IEEE 802 standardsIEEE 802 standards, are widely used in the utility network. The Wi-SUN standard, built on IEEE 802.15.4 SUN technology, is a successful and widely deployed example used for metering networks. There are a number of characteristics that make the mesh topology favorable in some deployment situations.

Mesh topology extends the range of the network well beyond the range of a single radio link. Multi-hop delivery can assist in reaching endpoints in poor RF environments, as adjacent neighbors will forward messages to the hard-to-reach node. This in turn allows greater network range with low power radios that can operate in license-exempt frequency bands.

In dense deployment scenarios, mesh topology can allow reducing the transmit power and/or increasing the symbol rate, which are both measures that can reduce interface from and with other nodes by reducing the interference footprint. An inherent tradeoff in multi-hop network topologies is that forwarding will, in some cases, increase latency. In interference limited environments, use of mesh topology can improve delivery reliability, which will reduce retransmission delays. Similarly, the resistance to interference improves delivery reliability, which can improve the effective throughput as well, as retransmission caused by collisions increases the spectrum bandwidth required to deliver the message.

In a wireless system, rate (throughput) and range are inversely related if all other factors are equal. A lower rate can operate over a longer range. In multi-hop (relay or mesh networks), there is also an inverse relationship between latency and range. If range is extended by forwarding packets through a mesh or multi-hop network, the latency increases proportionally to the number of hops. This topic is presented in greater depth in NISTIR 7761 V2 (2013), Section 6.1 [2].

# Applications for Smart Grid

The electric power system is logically separated into three main domains; these domains include Generation, Transmission, and Distribution. Among the categories of Smart Grid applications are Advanced Metering Infrastructure (AMI) and Distribution Automation (DA).

## AMI

AMI improves utility metering by providing two-way communication, which enables the following features: Utility service outage and restoration management, meter reading, demand response, load management, remote service disconnection/re-connection, and service pricing capabilities (including Real Time Pricing, Time of Use pricing, and Critical Peak pricing). For more information, refer to NISTIR 7761 V2 (2013) [2].



Figure 2: High level example of an AMI system

## DA

DA extends intelligent control to the distribution system that includes the following capabilities: Voltage Optimization, Load Reduction/Optimization, system fault detection and remediation, and SCADA. For more information, refer to NISTIR 7761 V2 (2013) [2].

## Application requirements for network communications

### Security

The security of power grid communications is vital from a national security point of view. Security protocols and encryption need to be certified by international bodies. Security protocols need to be interoperable, widely deployed, and have years of testing and deployment in the field. IEEE 802.1X link layer security is based on FIPS approved technologies and defines the encapsulation of Extensible Authentication Protocol (EAP) over an IEEE 802 network. In addition to providing port-based authentication to a server, the 802.1X protocol provides a secure mechanism for transferring keys used for link-layer encryption. IEEE 802 link layer security has been widely deployed in enterprise environments where security of corporate data is of utmost importance. These protocols have been vetted by a large number of security professionals.

### Non-mains powered operations (for some devices)

There are many Smart Grid applications that require non-mains powered operation, for example, certain types of sensors may not have access to the mains power in a cost-effective manner or need to operate during power outages.

Many IEEE 802 standards have been developed with energy constrained devices in mind. This focus enables the implementation of networked devices that operate for years from small capacity primary cell batteries. Some IEEE 802 standards have been developed with the goal to work from energy harvesting as well.

### Coverage requirements

In general, Smart Grid systems need to provide network services throughout the utility’s service area. To do this, Smart Grid systems need to support a hierarchy of networks that have different link distance requirements. In addition, the network needs to be robust enough to allow end point devices to reach the gateways. There are a variety of IEEE 802 standards for the networks that implement these requirements.

To achieve the required coverage, IEEE 802 standards provide a variety of solutions

* Multi-hop, non-deterministic networks (e.g., wireless mesh networks and bridged wired networks).
* Star networks with a base station and relatively long-distance wireless links
* A variety of physical layers with different data rates (e.g., modulation, coding, etc.)
* Fiber links when right of way is available

While 80% of the people lie within 20% of the service territory, AMI networks need to service 100% of the meters. Multi-hop networks can be used for hard-to-reach meters to get 100% coverage.

For resource constrained devices, multi-hop networks provide connectivity with low power usage. In some cases, constraints on the allowed transmit power levels for wireless networks restrict the practical link distance. In these cases, multi-hop networks may offer a solution. Multi-hop networks, both wired and wireless, also allow resiliency during the failure of nodes in the system.

Communications over fiber or wireless gives resilience to induced voltage differences when operating in proximity to high voltages.

For connectivity within a single facility, e.g., intra-substation networking and the head end, IEEE 802.3 (Ethernet) provides a cost-effective solution.

### Advantages of IEEE 802 networks

Utilities expect that deployments of Smart Grid networks will have a minimum lifetime of ten (10) to twenty (20) years. In general, IEEE 802 standards support backward-compatibility, as continuous improvements are adopted. This framework assists in preventing the need for "fork-lift upgrades" in the field. IEEE 802 has more than forty years of history in creating successful, backward-compatible standards.

Network and devices upgrades are achieved via incremental implementations that support multiple generations of IEEE 802 standards in the same network. In addition, the process in IEEE 802 includes the evaluation of coexistence with existing networking technologies to ensure good performance.

### Other Standards and Non-802 Networks

Reference to white paer on 802 Architecture

Point out adoption of Private LTE and 5G

Use of proprietary p-mp wireless

Need for Peer to Peer communications for dynamic reconfiguration of microgrids and outage recovery. No existing standards provide long range (> 1 km ) connectivity on a peer to peer topology. Possible adaptation of 802.16t?

# Conclusions

The IEEE 802 standards family provides a foundation of connectivity that network and application layer protocols can build upon to form a flexible, interoperable ecosystem serving a variety of applications.

The IEEE 802 family is well established in many utility communications applications. IEEE Std. 802.3 (Ethernet) finds broad application in enterprise LANs and intra-substation networks. IEEE Std. 802.16 and 802.15.4 (SUN PHY) are deployed for utility field area networks. IEEE Std. 802.15.4 (DSSS PHY) and IEEE Std. 802.11 (Wi-Fi) are used for Home Area Networks and other customer premises networks for energy management, load control, and automation.

The variety of IEEE 802 standards address the different requirements for different tiers of an integrated utility network (performance, range, latency, etc.) The unified architecture enables integration across the network. The architecture and design principles of IEEE 802 have been extended into other standards that have utility application, such as the IEEE1901 PLC standards, enabling broader integration.

IEEE 802 standards backward compatibility between generations, protecting investments and allowing incremental upgrades, while evolving to address new requirements.

In summary, IEEE 802 standards provide a platform to support the communication requirements of diverse applications across the range of utility operations, and other devices in support of the SmartGrid, eHealth industry, intelligent transportation systems, smart city applications, and general Internet of Things (IoT).

# Citations

1. “IEEE 802 recommendations on IEEE 802 related Smart Grid standards”, <https://mentor.ieee.org/802.24/dcn/12/24-12-0033-04-0000-package-of-802-smart-grid-standards.docx>
2. NISTRIR 7761 V2, Guidelines for Accessing Wireless Standards for Smart Grid Applications.