|  |
| --- |
| Ch 7.7.7 amendment: Detail Procedure for Monitoring |
| Date: 2018-03-20 |
| **Authors:**  |
| Name  | Affiliation  | Phone  | Email  |
| Hao Wang | Fujitsu |  | wangh@cn.fujitsu.com |
|  |  |  |  |
|  |  |  |  |
| **Notice:**This document does not represent the agreed view of the OmniRAN TG It represents only the views of the participants listed in the ‘Authors:’ field above. It is offered as a basis for discussion. It is not binding on the contributor, who reserve the right to add, amend or withdraw material contained herein.  |
| **Copyright policy:**The contributor is familiar with the IEEE-SA Copyright Policy <<http://standards.ieee.org/IPR/copyrightpolicy.html>>.  |
| **Patent policy:** The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://standards.ieee.org/guides/bylaws/sect6-7.html)> and <[http://standards.ieee.org/guides/opman/sect6.html#6.3](http://standards.ieee.org/guides/opman/sect6.html)>. |

Abstract

This document provides an amendment proposal to resolve comment #102 of DCN-18-0006-04.

# Chapter

## Accounting and monitoring

### Detail procedures

#### Monitoring

Similar to the procedures described in clause 7.7.7.2, the performance of the access network should be monitored during the period of use session.

As shown in Figure x, the ANC may send the monitoring (start) request towards the NMS for authorization of the monitoring task. Upon receiving the request, the NMS should reply the monitoring configuration parameters as a response to the ANC, if permitted. Then, the monitoring point will be setup on the corresponding network element, such as the NA, and monitoring process will be performed afterwards.

The network element may report the measurement results periodically or once at the end of monitoring process according to the specific configuration. The results may be mediated to fill up the required format and forwarded to the NMS for further processing.

The monitoring process may be terminated upon request, or caused by timeout or by the end of the user session.



Figure x: Procedure of monitoring