IEEE P802.15
Wireless Specialty Networks

|  |
| --- |
| 143th IEEE 802.15 WSN MEETING**802.15 IG NEXT GEN SUN PHY Minutes July 2023 Hybrid Mtg** |
| Date: 2023-07-11 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Thomas Almholt | Texas Instruments | 12500 TI BlvdDallas, Texas |  | talmholt@ti.com |
|  |  |  |  |  |

Abstract

# This document contains the IG notes from the July 10-13, 2023 Plenary meeting

**Tuesday, 11th July 2023, 16:00 (Berlin) IG Next Gen SUN PHY PM#2**

1. The meeting was recessed early due to a scheduling issue with the rooms at the site. No business was conducted during this meeting

**Wednesday, 12th July 2023, 16:00 (Berlin) IG Next Gen SUN PHY PM#2 1**

1. The IEEE 802.15 IG meeting was called to order by the Chair.

1. The Chair reviewed the IEEE-SA patent policy, copyright policy, logistics, and reminders, including meeting guidelines and attendance recording procedures.
2. Agenda for Tuesday PM2 meeting was presented by Chair
	* Approved by unanimous consent
3. Reviewed Call to action email that was sent by WG Chair on May 31st, 2023
4. Call to action had three technical submission:
	* Henk de-Ruijter, Silabs
		+ 64-QAM extension for the SUN OFDM PHY (15-23-0389-00-04ad)
		+ Preamble proposal for the SUN OFDM-LR PHY (15-23-0391-00-04ad)
	* Hiroshi Harada, Kyoto University. (15-23-0390-00-04ad)
		+ latest research and proposal for SUN extension related to SUN-OFDM and SUN-FSK
5. Technical presentation from by each submitter and good technical discussions on each topic presented.
6. Discussion on asking the WG chair to become a Study Group with the following objective
	* Additional improvement to the SUN-OFDM specification with a particular focus on long-range communication in highly congested environments
		+ Data rates of 1 - 50kbps
		+ RX Sensitivity of approximately -120dBm @ 1% PER 64 bytes (payload)
		+ Consider collision mitigation techniques
		+ Compliant with FCC 15.247 “digital modulation techniques”
		+ Focus on symmetrical communication
	* Additional higher data rate options for SUN-OFDM and improved robustness
		+ Introduction of 64/256 QAM to the SUN-OFDM specification (more advanced error codecs)
		+ Improve performance low data option of existing SUN-OFDM (maybe improving synch)
		+ Additional extension to the SUN-FSK specification including increased channel BW ( specifically Japan )
		+ Improve coexistence in general as this is an unlicensed band
	* Additional frequency range for SUN PHY
		+ Add new frequencies that have been added to regional regulation
7. Formal text to WG chair was developed
8. Meeting was adjourned

================================= END ==============================