**IEEE 802.24**

**Smart Grid TAG**

|  |  |  |
| --- | --- | --- |
| Project | IEEE 802.24 Smart Grid TAG | |
| Title |  | |
| Date Submitted | [March 20, 2013] | |
| Source | [Khurram Waheed] [Freescale Semiconductor] | Voice: [] Fax: [ ] E-mail: [khurram.waheed@freescale.com] |
| Re: | [] | |
| Abstract | [Text for inclusion of O-QPSK PHY from IEEE Std. 802.15.4-2011 in the list smart grid IEEE 802.15 standards] | |
| Purpose | [] | |
| Notice | This document has been prepared to assist the IEEE 802. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by IEEE 802.24. | |

# Introduction

The following section provides the text for inclusion in Section 4.4 of the document (#24-12-0033-XX) defining a list of 802 and related standards that provide solutions for smart grid Networks.

# Proposed text

*The proposed text in provided in the following paragraph. The editor is requested to make any necessary modifications to adapt the proposed text to the targeted document:*

**802.24-WG15-3**

* **O-QPSK PHY in IEEE Std 802.15.4™-2011: Low-Rate Wireless Personal Area Networks (LR-WPANs)**IEEE Std 802.15.4-2011 defines the physical layer (PHY) and medium access control (MAC) sublayer specifications for low-data-rate wireless connectivity with fixed, portable, and moving devices. O-QPSK PHY specified in Clause 10 of this standard defines a direct sequence spread spectrum (DSSS) PHY employing offset quadrature phase shift keying (O-QPSK) modulation. O-QPSK PHY is widely deployed for home area networking and smart metering applications.