IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions For CID 6051 |
| Date: 2014-11-03 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham | Qualcomm | 5775 Morehouse Dr., San Diego, CA 92121 | +1 858 651 6107 | sabraham@qti.qualcomm.com |
| George Cherian | gcherian@qti.qualcomm.com |

Abstract

This document provides proposed resolution for CIDs 6051

**8 Frame Formats**

**8.4 Management and Extension frame Body Components**

**8.4.2 Elements**

* FILS Indication element

***Change Figure 8-574n to the following***

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | IP Address Type  | Subnet ID Token (conditional) | Public Key Entry |
| Octets | 1 | 1 | Variable |

**Figure 8-574n—Format of Public Key Information field**

***Add the following figure below Figure 8-574n***

|  |  |  |
| --- | --- | --- |
|  | IP Address Type  | Reserved |
| Bits | B0 B2 | B3 B7 |

 **Figure 11-A12—Format of IP Address Type in Public Key Information field**