IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB204 Comment Resolutions for CID 6225 | | | | |
| Date: 2015-01-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei WANG | InterDigital Communications, Inc. | 2 Huntington Quadrangle Melville, NY 11747 |  | xiaofei.wang@interdigital.com |
| Joseph LEVY | InterDigital Communications, Inc. | 2 Huntington Quadrangle Melville, NY 11747 | +1.516.835.9353 (m) | joseph.levy@interdigital.com |

Abstract

This document provides proposed text changes to the draft as a result for comment resolutions for CID 6225. This comment addresses Clause 8.6.24. The baseline for this comment resolution document is 802.11ai Draft 3.1.

**Red Lined Text Changes for the Proposed Resolutions:**

**CID 6225**

**Instructions for Editor: please modify the text of 8.6.24, from Line 1, Page 75 to Line 20 Page 75 with the following changes:**

* FILS Action frames

The FILS Action frame is used for FILS operation after the non-AP STA has associated with the AP. A FILS Action field, in the octet immediately after the Category field, differentiates the FILS Action frame formats. The defined FILS Action frames are listed in Table 8-405a (FILS Action field values).

|  |  |
| --- | --- |
| * FILS Action field values | |
| FILS Action field value | Description |
| 0 | FILS Container [13/1358r3][CID 4882] |
| 1-255 | Reserved |

***Insert new clause as follows:***

* FILS Container Action frame [CID 6920]

**References:**

1. **IEEE 802.11-14/1351r15, TGai LB204 comments on D3.0, Marc Emmelmann, November 2014**
2. **IEEE P802.11ai™/D3.1, November 2014**