IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution CID 10024 | | | | |
| Date: 2015-10-15 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham | Qualcomm | 5775 Morehouse Dr.  San Diego, CA 92129 | +1-858 651 6107 | sabraham@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

This submission addresses CIDs 10024

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Comment | Proposed Change | Proposed Resolution |
| 10024 | Wrong formula. | Remove ", 0, 15)". | Revised: Accept changes given in 11-15-1295/r2 |

***Instruct the editor to modify section 10.47.4 as indicated:***

**10.47.4 FILS authentication and higher layer setup capability indications**

***Change Lines 23-28 of Page 124 with the following***

H = L(CRC32-(~~x~~ ToLowerCase(D)~~)~~,0,16)~~,0,15)~~ (2)  
where:  
CRC-32(x) is calculated by using G(x) function defined in 8.2.4.8 (FCS field). ~~, where x is ToLowerCase(D)~~