### IEEE P802.11 Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11ax D0.1 Spec Texts for MU-RTS HE MU PPDU Restriction | | | | |
| Date: 2016-07-24 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Po-Kai Huang | Intel Corporation | 2200 Mission College Blvd, Santa Clara, CA 950542200 |  | po-kai.huang@intel.com |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes spec texts for motion passed in 16/648

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revise based on the editorial comment from Mark. The difference are marked with green.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax D0.1 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax D0.1 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

**Discussion:**

In 16/648, the following motion has passed to restrict MU-RTS from being carried in HE MU PPDU*.*

*MU-RTS shall not be carried in an HE MU PPDU*

Propose texts in the spec for this motion.

**Propose:**

Propose spec texts in 11ax TG draft 0.1 for the following motion.

*MU-RTS shall not be carried in an HE MU PPDU*

***TGax editor: Add the Paragraph on page 40 line 62 as the following:***

An MU-RTS frame shall not be carried in an HE MU PPDU.