### IEEE P802.11Wireless LANs

|  |
| --- |
| 11ax D1.0 MAC Comment Resolution for  |
| Date: 2017-09-10 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Chao-Chun Wang | MediaTek Inc | 2840 Junction Ave, San Jose, CA 95134, USA |  | Chaochun.wang @mediatek.com |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for comments of TGax Draft 1.0 and the proposed change is for TGax Draft 1.4

CIDs: 3050, 5847, 7384, 8315

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax D1.0 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax D1.0 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3050 | 105.28 | 9.6.29.4 | Incorrect text | This paragraph describes the request operation - instead it should describe the response operation | Revised: The comment was addressed in CID 3038 and the changes are included in draft 1.4 . Please see 9.6.30. |
| 5847 | 105.29 | 9.6.29.4 | Description of Quiet Time Period Response frame format is not correct: it is the response to the Quiet Time Request frame received, not the request to the Quiet Time Reqeust frame received | Change: "to request" to "to response" | Revised: The comment was addressed in 3050 |
| 7384 | 105.28 | 9.6.29.4 | The text is confusing. It mentions a request in the response frame. | Clarify the meaning of the frames | Revised: The comment was addressed in 3050 |
| 8315 | 99.44 | 9.6.8.34 | If AP supports QAB, the Quiet Time Period action frame may be required. | Insert changes to QAB frame format if required | Rejected: The PL number is inconsistent with clause number. The correct one is 9.6.9.16. The comment is rejected since Quiet Time Period protocol is to support all peer-to-peer operations and not just TDLS. If TDLS also want to take advantage of the protocol, it will be a new update to the TDLS protocol. |

**Discussion:**

3050 Duplicated: The comment was addressed in CID 3038 and the changes are included in draft 1.3

5847 Duplicate: 3050

7384 Duplicate: 3050

8315 Rejected: The PL number is inconsistent with clause number. The correct one is 9.6.9.16. The comment is rejected since Quiet Time Period protocol is to support all peer-to-peer operations and not just TDLS. If TDLS also want to take advantage of the protocol, it will be a new update to the TDLS protocol.

**Propose:**

No change to the draft 1.4.

***TGax Editor: None***

###