IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed resolution to CID 1001, 1002 from the second recirculation Sponsor Ballot |
| Date: 2017-08-10 |
| Author(s):  |
| Name | Company | Address | Phone | Email |
| Jiamin Chen | Huawei/HiSilicon |  |  | Jiamin.chen@mail01.huawei.com |
|  |  |  |  |  |

 Abstract

This document proposes resolutions to 2 CIDs on TGaj D7.0: 1001, 1002.

**Revision History**

R0: Initial version.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Type | Comment | Proposed Change | Remark |
| 1001 | 9.4.2.232.5 | 219 | 42 | T | The value of Mse should be "4" rather than "7" when the Nss is 4. | Change the value of Mse from "4" to "7" when the Nss is 4. |  |

Proposed resolution: **Accepted.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Type | Comment | Proposed Change | Remark |
| 1002 | 25.6.8.14.2 | 242 | 17 | T | "Figure 25-27-NDP format" The title of Figure 25-27 needs to be more specific. | Change the title of Figure 25-27 from "NDP format" to "CMMG NDP format". |  |

Proposed resolution: **Accepted.**