IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolutions on Clause 28.3.3.4 (Pilot subcarriers) | | | | |
| Date: 2017-09-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Junghoon Suh | Huawei Tech | 303 Terry Fox Dr, Kanata, ON K2K 3J1, Canada | +1-613-595-1900 | junghoon.suh@huawei.com |

Abstract

This submission proposes a comment resolution for the comment # 10374 on Clause 28.3.3.4 of TGax D1.4:

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 10374 | 28.3.3.4 | 236.37  (based on D1.0) | All pilot subcarriers are at the even indices enumerated in Table 28-7 (Pilot subcarrier indices). | word "even" is redundant | Rejected—  It is not redundant, but helps further clarify the statement. |

**References:**

1. **IEEE P802.11axTM/D1.4, Aug 2017**