IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution of 10.38.2 CIDs |
| Date: 2018-02-27 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Li-Hsiang Sun | Interdigital |  |  | Lihsiang.sun@interdigital.com |
| Xiaofei Wang |  |  |  |  |
| Rui Yang |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions to 1483, 1546, 1547 CIDs.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Prposed change** | **Proposed resolution** |
| 1483 | 10.38.2.5 | 149.18 | Do EDMG STAs use DMA antennas? | Clarify | RejectedThroughout the 11ay draft, antennas used by EDMG STAs are called DMG antennas, e.g. 9.4.2.250.3 “Number of DMG Antennas” subfield |
| 1546 | 10.38.2.4 | 148.34 | "DMG Antenna Select MSB" subfield is mssing | 1. L34P148: change "the DMG Antenna Select subfield" to "the DMG Antenna Select and DMG Antenna Select MSB subfields"2. L39P148: change "Sector Select MSB and DMG Antenna Select fields" to "Sector Select MSB, DMG Antenna Select and DMG Antenna Select MSB subfields" | Accepted |
| 1547 | 10.38.2.5 | 149.5 | DMG Antenna Select MSB field is mssing | 1. L5P149: change "Sector Select MSB field and DMG Antenna Select field" to "Sector Select MSB field, DMG Antenna Select field and DMG Antenna Select MSB field"2. L14P149: change "Sector Select MSB field and DMG Antenna Select field" to "Sector Select MSB field, DMG Antenna Select field and DMG Antenna Select MSB field" | RevisedAgreed with commenter. Change field to subfield1. L4P149: change "by the value of the Sector Select field, Sector Select MSB field and DMG Antenna Select field" to " by the value of the Sector Select subfield, Sector Select MSB subfield, DMG Antenna Select subfield and DMG Antenna Select MSB subfield" 2. L14P149: change " Sector Select field, Sector Select MSB field and DMG Antenna Select field" to " Sector Select subfield, Sector Select MSB subfield, DMG Antenna Select subfield and DMG Antenna Select MSB subfield" |