IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB232 CID1243 – Proposed Comment Resolution | | | | |
| Date: 2018-09-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Marc Emmelmann | SELF;  Koden-TI | Berlin, Germany |  | emmelmann@ieee.org |
| Hitoshi Morioka | SRC Software | 2-14-38 Tenjin, Chuo-ku, Fukuoka 810-001 JAPAN |  | hmorioka@src-soft.com |

Abstract

Proposed comment resolution for CID 1243 (TGm LB232).


**CID 1243**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Clause Number(C)** | **Page** | **Comment** | **Proposed Change** |
| 1243 | 11.23.3.3.1 | 2207.37 | The use of the CAG (which is effectively ANQP response caching) in a STA can be used in any STA, not just a FILS STA. To some extent CAG is independent of FILS, even though it was introduced in the 11ai roll-up. In addition this clause is the ANQP behavior clause, which should have no dependancy on FILS. | Change the text "A FILS STA" to "A STA" at the start of the cited sentence |

Discussion

Note: P2207.37 refers to D1.0 which is in D1.4 on page 2366

Context: D1.4 P2366



The comment correctly identifies that the cited clause does not only relate to FILS but to a STA in general.

Proposed Resolution:

Accept.