IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Spatial Reuse ad hoc group September 2018 minutes | | | | |
| Date: 2018-09-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Laurent Cariou | Intel |  |  | [Laurent.cariou@intel.com](mailto:Laurent.cariou@intel.com) |
| Guido R. Hiertz | Ericsson | Ericsson Allee 1 52134 Herzogenrath Federal Republic of Germany | +49-2407-575-5575 | hiertz@ieee.org |

Abstract

This document contains the meeting minutes of the IEEE 802.11ax ad hoc group on spatial reuse (SR) that met on 2018-09-10.

Chairman of the 802.11ax Spatial Reuse (SR) ad hoc group calls the meeting to order.

The Chairman reminds all attendees to record attendance for this session. The Chairman reviews the IEEE IPR patent policy. The Chairman calls for potentially essential patent claims. There is no response to his question. The Chairman reminds all attendees to identify themselves and their affiliations each time they speak for the first time on a meeting day.

The Chairman reviews the agenda for this week’s IEEE 802.11ax Spatial Reuse ad hoc group meeting sessions.

Laurent Cariou presents 11-18/1495r3.

Strawpoll:

Do you agree on resolutions to CIDs 16516, 15657, 16512, 15176 in doc 11-18/1495r3.

Y: 22, N: 0, A: 3

Mat Fischer presents 11-18/1410r0.

Comment: More discussion on power measurement on L-SIG. Defer SP to accommodate change.

Graham Smith presents 11-18/1531r3

Strawpoll:

* **Resolve CID 15652 to allow an AP to include the OBSS\_PD Margin and to allow a STA to adjust its ODSS\_PD level in accordance with**

*OBSS\_PDlevel* = *RSSI\_* *beacon* – *OBSS\_PD\_Margin*

*With OBSS PDmin <OBSS\_PDlevel < OBSS\_Pdmax*

Note to Assignee: CID proposed accepting text in 18/0617r2 which referenced D2.2 18/0617r3 is now posted referring D3.0

Y: 8, N:8, A:8

Meeting adjourned for the week