IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Suggested comment resolution for CID 2579 on REMmd D2.0 | | | | |
| Date: 2019-07-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Marc Emmelmann | Self | Berlin, Germany |  | emmelmann@ieee.org |
| Hitoshi Morioka | SRC Sorftware | Fukuoka, Japan |  | hmorioka@src-soft.com |
| Hiroshi Mano | KDTI | Tokyo, Japan |  | mano@koden-ti.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# Abstract

This submission presents a suggested comment resolution for CID(s) 2579 on REVmd D2.0

Table of Contents

[Abstract 1](file:////Users/mem/Documents/Privat/Projects/802.11-TGm/REVmd-D2-Fils_comments/11-19-1253-00-000m-Suggested%20comment%20resolution%20for%20CID%202579%20on%20REMmd%20D2.0.docx#_Toc14081587)

[Comment 3](#_Toc14081588)

[Discussion 3](#_Toc14081589)


[Proposed Resolution 4](#_Toc14081590)

# Comment

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **LB** | **Draft** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** |
| 2579 | 236 | 2 | 2133.00 | 7 | 11.1.4.3.4 | "A FILS STA may choose not to respond to Probe Request frames from a FILS STA addressed to broadcast address if the responding STA receives an acknowledged probe response addressed to the requesting STA containing the SSID of the responding STA." -- it's not clear which is the "responding STA" here since this is about a FILS STA choosing not to respond! | Change to "A first FILS STA may choose not to respond to Probe Request frames from a second FILS STA addressed to the broadcast address if the first STA receives an acknowledged probe response addressed to the second STA containing the SSID of the first STA." |

# Discussion

Context of the comment (D2.0 P2133)



The comment identifies a potentially confusing wording and provides a suggested rewording.

# Proposed Resolution

ACCEPT