IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolution D0.3 Section 31.1 | | | | |
| Date: 2020-09-04 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| James Lepp | BlackBerry |  |  | jlepp@ieee.org |
|  |  |  |  |  |

Abstract

Comment Resolution for 802.11bd D0.3 CID 24, 90

Revision 0: 2020-07-31

Revision 1: posted after teleconference strawpoll 2020-09-04

**Comments:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Proposed Resolution** |
| 24 | 22.05 | 5 | 31 | Add MLME primitive and/or MIB to turn range extension (MCS 10) on or off. | Add MLME primitive and/or MIB to turn range extension (MCS 10) on or off. | Rejected: MCS 1-10 are mandatory including MCS10. |
| 90 | 22.20 | 20 | 31.1 | This sentence seems too vague. What this sentence means is that the functions in Clause 31 supersedes the functions in Clause 10 and 11 when there is conflict between the functions. Please rephrase this to reflect this meaning. | As shown in the comment. | Reject: The text is identical to that of 11ax D6.0 and is considered clear. |

**9/4/2020 Straw Poll: Do you agree to reject CID90 and keep the original text? 12Y/0N/5A/1NR**