IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11be Spec text for Motion #150, SP #372 (disallowing static frag in MLO) | | | | |
| Date: 2021-04-18 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm |  |  | appatil@qti.qualcomm.com |
| George Cherian |  |  |  |
| Alfred Asterjadhi |  |  |  |
| Duncan Ho |  |  |  |
| Yanjun Sun |  |  |  |
| Gaurang Naik |  |  |  |  |

Abstract

We propose the draft text related to motion 150, SP 372 (related to disallowing static fragmentation) to help the creation of TGbe draft D1.0.

Revisions:

* Rev 0: Initial version of the document.

**The proposed texts is based on the following motion:**

802.11be shall disallow static fragmentation in MLO.

[Motion 150, #SP372, [92] and [227]]

***TGbe editor: Please insert the following (new) subclause to clause 35.3 as shown below:***

**35.3.xx Fragmentation in multi-link operation**

A STA affiliated with an MLD shall not use the fragmentation procedure described in 10.4 (MSDU, A-MSDU, and MMPDU fragmentation).