IEEE P802.11
Wireless LANs

|  |
| --- |
| CID 3053 for Midambles |
| Date: 2022-01-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Rui Cao | NXP | 350 Holger Way, San Jose,CA |  | rui.cao\_2@nxp.com |

Abstract

This submission proposes resolutions for CID 3053 received on Section 32.3.9.9 (Midambles) in TGbd D3.0.

Revisions:

* r0: initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 3053 | 32.3.9.9 | 107.45 | N\_SYM is not defined in 32.3.9.4. | Please refer the correct subclause. | RevisedTGbd editor: please replace P107L45 with “where N\_SYM is the total number of data symbols in the Data field, and is given in Clause 21.3.10.5.4 (LDPC coding) (computed using Equation (19-41) in step d) of Clause 19.3.11.7.5 (LDPC PPDU encoding process)).“ |

*Discussions:*

**

**

**