IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution for CID related to Status Code field | | | | |
| Date: 2022-02-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jiin (Namyeong) Kim | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea |  | jiin.kim@lge.com |
| Insun Jang | LG Electronics |  | insun.jang@lge.com |
| Sunhee Baek | LG Electronics |  | sunhee.baek@lge.com |
| Jinsoo Choi | LG Electronics |  | js.choi@lge.com |

Abstract

This document proposes resoulution for CIDs 7376 related Status Code field.

Revisions:

* Rev 0: initial version of the document

***TGbe editor: Please note that baseline is 11be D1.4***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 7376 | 110/51 | 9.4.1.9 | The status code "DENIED\_STA\_AFFILIATED\_WITH\_MLD\_WITH\_EXISTING\_MLD\_ASSOCIATION" could be improved, as the term "MLD" is duplicated. | Change the cited status code to "ASSOCIATION-DENIED-STA-AFFILIATED-WITH-MLD" | **Rejected.**  This is not duplicated meaning. That menas the non-AP MLD with which the non-AP STA is affiliated was already associated with the AP MLD. |

1. **Proposed spec text**

***TGbe editor: the following spec text is not for comment resolution, just for reference to explain.***

**9.4.1.9 Status Code field**

Table 9-50 Status codes

|  |  |  |
| --- | --- | --- |
| **Status code** | **Name** | **Meaning** |
| <ANA> | DENIED\_STA\_AFFILIATED\_WITH\_MLD\_WITH\_EXISTING\_MLD\_ASSOCIATION | Association denied because the requesting STA is affiliated with a non-AP MLD that is associated with the AP MLD. |
| <ANA> | NSEP\_DENIED\_UNAUTHORIZED | NSEP priority access denied because the non-AP MLD or non-AP EHT STA is not authorized to use the service. |
| <ANA> | NSEP\_DENIED\_OTHER\_REASON | NSEP priority access denied due to reason outside the scope of this standard. |
| <ANA> | DENIED\_TID\_TO\_LINK\_MAPPING | Request denied because the requested TID-to-link mapping is unacceptable. |
| <ANA> | PREFERRED\_TID\_TO\_LINK\_MAPPING\_SUGGESTED | Preferred TID-to-link mapping suggested. |
| <ANA> | DENIED\_EHT\_NOT\_SUPPORTED | Association denied because the requesting STA does not support EHT features. |