### IEEE P802.11Wireless LANs

|  |
| --- |
| 11be D1.0 CR for remaining CIDs in 6-3 |
| Date: 2022-03-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Zhiqiang Han | ZTE Corporation |  |  | han.zhiqiang1@zte.com.cn |
| Yan Li | ZTE Corporation |  |  | li.yan16@zte.com.cn |

Abstract

This submission proposes resolutions for the following 5 CIDs:

CID : 7757,7758,5648,6167,7381

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe D1.4 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe D1.4 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 7757 | Yanchao Xu | 51.19 | 6.3.3.2.2 | (Probe Request variant) Multi-Link Element should be inlcuded In MLME-SCAN.request | as comments | RejectedThe group discussed the comment and proposed resolution and could not come to consensus on a set of changes that would satisfy the commenter |
| 7758 | Yanchao Xu | 52.01 | 6.3.3.3.2 | (Basic variant) Multi-Link Element of peer MLD should be inlcuded In MLME-SCAN.confirm | as comments | RejectedThe group discussed the comment and proposed resolution and could not come to consensus on a set of changes that would satisfy the commenter |
| 5648 | Joseph Levy | 66.36 | 6.3.39.2.1 | What is a peer MLD? How can an MLD be associated with an MLD? Association is a concept that includes entities beyond the MLD (BS, ESS, DS). A non-AP MLD does not associated with an AP MLD, as association is with a BS or an ESS and involves the DS. Note: this phase "peer MLD" occurs in multiple location (66.45, 66.56, 67.1, 67.22, 67.31, 67.41, 161.14, 189.2, 192.40, 205.41, .... a total of 22 instances). All occurrences should be addressed. | Define what a peer MLD is and how this relates to association. Correct the statement that the MLD is some how associated to the "peer" MLD. Make these changes at all location where this phrase is used. | **Rejected**The group discussed the comment and proposed resolution and could not come to consensus on a set of changes that would satisfy the commenter |
| 6167 | Michael Montemurro | 66.36 | 6.3.39.2 | The STA authenticator would have no state associated with an MLD association. | At 66.36 and 66.45, change "or be sent to an affiliated STA of the specified peer MLD to which the MLD is associated." to "or be sent to an the specified peer MLD to which the MLD is associated."At 66.56, change "The STA then attempts to transmit this to the peer STA with which it is associated or a STA affiliated with the MLD attempts to transmit this to another STA affiliated with the peer MLD with which the MLD is associated on the corresponding link." to "The STA or MLD then attempts to transmit this to the peer STA, or MLD with which it is associated on the corresponding link."At 67.22 and 67.31, change "or to a STA affiliated with the peer MLD" to "or MLD"At 67.39, change "The STA then attempts to transmit this to the STA indicated by the PeerSTAAddress parameter or a STA affiliated with the MLD then attempts to transmit this to a STA affiliated with the peer MLD indicated by the PeerSTAAddress parameter." to "The STA or MLD then attempts to transmit this to the STA or MLD indicated by the PeerSTAAddress parameter." | **Rejected****The group discussed the comment and proposed resolution and could not come to consensus on a set of changes that would satisfy the commenter** |
| 7381 | Stephen McCann | 66.36 | 6.3.39.2.1 | Regarding the text "...be sent to an affiliated STA of the specified peer MLD to which the MLD is associated.", is the MLD associated to the affiliated STA or to the specified peer MLD? | Change the cited sentence extract to ""...be sent to an affiliated STA of the specified associated peer MLD." | RejectedThe group discussed the comment and proposed resolution and could not come to consensus on a set of changes that would satisfy the commenter  |