IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution for CID 3139 | | | | |
| Date: 2022-05-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Michael Montemurro | Huawei Technologies Co., Ltd | Toronto, Ontario, Canada |  | Montemurro.michael@gmail.com |

Abstract

This submission proposes a resolution to TGbc CID 3139 related to Draft P802.11bc D3.0.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Proposed Resolution** |
| 3139 | 80.17 | 10.2.7 |  | Need to provide an additional requirement to address the topic proposed in the Editor's note. | Commenter will bring a contribution proposing a resolution to this CID. |

***Discussion***

An Action was taken to provide a requirement to specify that EBCS data frames are not forwarded beyond the DS.

***Proposed Resolution based on D3.0***

Change the paragraph at p80.13 in P802.11bc 3.0 as follows:

Change "An EBCS STA follows the procedures defined in 11.55 (Enhanced Broadcast Services procedures) for the transmission and reception of EBCS traffic."

to

"An EBCS STA follows the procedures defined in 11.55 (Enhanced Broadcast Services procedures) for the transmission and reception of EBCS Data frames. EBCS Data frames shall not be forwarded beyond the DS."

NOTE: The cited clause in P802.11bc D3.0, 10.2.7, should be renumbered to 10.2.8 to align with REVme 1.x drafts.