IEEE P802.11  
Wireless LANs

|  |
| --- |
| **LB266 CR for 9.2.4.5** |
| **Date:** 2022-07-25 |
| **Author(s):** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Jinyoung Chun | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea |  | jiny.chun@lge.com |
| Dongguk Lim |  | dongguk.lim@lge.com |
| Eunsung Park |  | esung.park@lge.com |
| Jinsoo Choi |  | js.choi@lge.com |
| Insun Jang |  | insun.jang@lge.com |

Abstract

This submission proposes a resolution for 4 CIDs: 10967, 12236, 12237, and 12238

All the changes are based on P802.11be D2.0.

Revisions:

* Rev 0: Initial version of the document.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 10967 | 9.2.4.5.6 | 121.34 | Need to fix a typo: "STA" instead "STAs" | As in comment | Accepted |
| 12236 | 9.2.4.5.4 | 120.21 | The Table 9-13 "Other conditions" revised sentence does not read well and requires the use of a ":" and a ";". | Change the sentence to "Bit 6 of the Frame Control field (see 9.2.4.1.3 (Type and Subtype fields)) is equal to 1 and the frame is not carried in either: an HE MU PPDU, HE SU PPDU or HE ER SU PPDU that contains a frame that solicits a response in an HE TB PPDU; or an EHT MU PPDU that contains a frame that solicits a response in an EHT TB PPDU." | Accepted |
| 12237 | 9.2.4.5.4 | 120.38 | The Table 9-13 "Other conditions" revised sentence does not read well and requires the use of a ":" and a ";". | Change the sentence to "Bit 6 of the Frame Control field (see 9.2.4.1.3 (Type and Subtype fields)) is equal to 0 and the frame is not carried in either: an HE MU PPDU, HE SU PPDU or HE ER SU PPDU that contains a frame that solicits a response in an HE TB PPDU; or an EHT MU PPDU that contains a frame that solicits a response in an EHT TB PPDU." | Accepted |
| 12238 | 9.2.4.5.4 | 121.09 | The Table 9-13 "Other conditions" revised sentence does not read well and requires the use of a ":" and a ";". | Change the sentence to "The frame is carried in either: an HE MU PPDU, HE SU PPDU or HE ER SU PPDU that contains a frame that solicits a response in an HE TB PPDU; or in an EHT MU PPDU that contains a frame that solicits a response in an EHT TB PPDU." | Accepted |