IEEE P802.11
Wireless LANs

|  |
| --- |
| 802.11bc LB 268 resolution for CIDs assigned to Abhi |
| Date: September 2, 2022 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm Inc. |  |  | appatil@qti.qualcomm.com |
| George Cherian |  |  |  |
| Jouni Malinen |  |  |  |

 Abstract

This submission proposes resolutions for CID 4012 submitted during LB 268 for 11bc D4.0

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Minor edits when the doc was presented on 9/6/22 telco

**3.2 Definitions specific to IEEE Std 802.11**

***TGbc Editor, please add a new definition as shown below in alphabetical order:***

[4012]**enhanced broadcast service (EBCS) proxy:** A logical component affiliated with an EBCS relaying STA, which might be collocated with the EBCS relaying STA, that can relay a higher layer protocol (HLP) payload carried in an EBCS UL frame received by the EBCS relaying STA to a destination specified in the frame, typically within an external network.

* + - * 1. **EBCS proxy operation**

***TGbc Editor: please update the following paragraphs in this subclause as shown below:***

[4012]