IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB271 Clause 35.3.16.8.3 Comment Resolutions | | | | |
| Date: 2023/03/28 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Stephen McCann | Huawei Technologies | Southampton, United Kingdom |  | [stephen.mccann@ieee.org](mailto:stephen.mccann@ieee.org) |

# Revision Notes

Abstract

This submission contains proposed comment resolutions to comments on P802.11be D3.0.

The following comment resolutions are proposed for CIDs:

16233, 16251 and 16252

|  |  |
| --- | --- |
| R0 | Initial revision |
|  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 16233 | 123.12 | 6.3.133.2.2 | Typo "EML operation" | Change "EML operation" to "EML operating mode". The same change also needs to be made at P123L54. | Accepted |
| 16251 | 332.14 | 10.3.2.9 | The sentence "the STA has received the RTS on a link that is a member of one or more of the MLD's NSTR link pairs" can be simplified. | Change the cited sentence to "the STA has received the RTS on a link that belongs to a NSTR link pair". | Revised: Change the cited sentence to "the STA has received the RTS on a link that belongs to an NSTR link pair". |
| 16252 | 332.17 | 10.3.2.9 | The sentence "another STA affiliated with the same MLD is a TXOP holder or TXOP responder on one of the other links that is a member of at least one of the NSTR link pairs of which the link on which the RTS was received is a member" can be simplified. | Change the cited sentence to "another STA affiliated with the same MLD, is a TXOP holder or responder on the other link of the NSTR link pair on which the RTS was received". | Accepted |