IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | MCS 14 | | | | | | Date: 2025-7-28 | | | | | | Author(s): | | | | | | Name | Affiliation | Address | Phone | email | | Youhan Kim | Qualcomm Technologies, Inc. |  |  | [youhank@qti.qualcomm.com](mailto:youhank@qti.qualcomm.com) | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |

Abstract

This submission proposes text update to clarify that MCS 14 is not used in UHR.

NOTE – Set the Track Changes Viewing Option in the MS Word to “All Markup” to clearly see the proposed text edits.

**Revision History:**

R0: Initial version.

## Background

During comment resolution on CIDs 358, 361 and 3707, TGbn decided not to define MCS 14 in UHR – see <https://mentor.ieee.org/802.11/dcn/25/11-25-0855-00-00bn-comment-resolution-for-38-5-parameters-of-uhr-mcs.docx>

Further clean up of MCS 14 from the TGbn draft was done in <https://mentor.ieee.org/802.11/dcn/25/11-25-0775-02-00bn-crs-on-new-mcss-for-subclause-38-5.docx>.

However, there is still one location which states that UHR supports MCS 14.

11bn D0.3 P342L13:

|  |
| --- |
| A black text on a white background  AI-generated content may be incorrect. |

This document proposes text update to remove the above reference to UHR MCS 14.

## Proposed Text Update

*Instruction to TGbn Editor: Update 11bn D0.3 P342L13 as shown below:*

UHR-MCS 15 is supported only with *Nss,u* = 1.

[End of File]