**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Proposed Resolutions for Flowchart Comments CID #R109, R110** | |
| Date Submitted | 6 July 2015 | |
| Source | [Charlie Perkins],  [Futurewei],  [2330 Central Expressway,  Santa Clara,  CA 95050] | Voice: [+1-408-330-4596]  Fax: [+1-408-330-5088]  E-mail: [charliep@computer.org] |
| Re: | 802.15.10 Consolidated Comment Entry Form, CIDs #R109, R110 | |
| Abstract | Provides a proposed resolution to CIDs #R109, R110 | |
| Purpose | To be used by the technical editor to apply the necessary changes to the draft to resolve CIDs #R109, R110 | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**Comments CIDs #R109, R110**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CID | Name | Page | Sub-clause | Line # | Comment | Proposed Change |
| R109 | Charlie Perkins | 38 | 5.4.1.3 | 38 | Lower-right "Forward packet" can also fail… | Lower-right "Forward packet" box needs a Failed arrow |
| R110 | Charlie Perkins | 38 | 5.4.1.3 | 41 | MAC layer function boxes can be coalesced | If convenient, move two center procedure up vertically |

**Resolution: AiP**

**CIDs #R109, R110:** The following revised flow diagram consolidates similar functions and improves the accuracy of the control flow.

* ***Replace Figure 20 as follows:***

