**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **TG4aa Coexistence Document** | |
| Date Submitted | 1 February, 2021 | |
| Source | [Kiyoshi Fukui, OKI, Japan] | E-mail: [fukui535@oki.com] |
| Abstract | Analysis on coexistence of 802.15.4aa with other 802 systems within the same spectrum bands. | |
| Purpose | To address the coexistence capability of 802.15.4aa. | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

# Introduction

TG4aa introduces operating modes to 802.15.4 supporting higher data rates in the 920MHz band. These new operating modes use GFSK modulation, which is one of the existing modulation methods. The higher data rates have the effect of increasing the signal bandwidth from the GFSK operating modes specified in 802.15.4 for the 920MHz band. The regulations governing the 920MHz band[B1] specify stringent requirements on devices to ensure efficient and equitable shared usage of the band. The regulation specifies a channel plan which also allows aggregation of channels, hence permitting varying signal bandwidths. It additionally specifies parameters for listen before talk, maximum transmit power levels and transmit duty cycle limits. The TG4g coexistence assurance document[B2], already provides a comprehensive analysis for coexistence in all bands, including 920MHz band. TG4aa adds no functionality, channel access requirements, or modulations beyond those used in 802.15.4. Therefore, the existing analysis in [B2] is sufficient to cover the TG4aa amendment.

# Bibliography

[B1] ARIB STD-T108, 920MHz-BAND TELEMETER, TELECONTROL AND DATA TRANSMISSION RADIO EQUIPMENT, (<http://www.arib.or.jp/english/html/overview/doc/5-STD-T108v1_3-E1.pdf>).

[B2] TG4g coexistence assurance document, (https://mentor.ieee.org/802.15/dcn/10/15-10-0668-05-004g-tg4g-coexistence-assurance-document-first-draft.pdf).