**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **LB225/D03 comment resolution -- CID 71** |
| Date Submitted | Oct 15, 2025 |
| Sources | Alex Krebs (Apple)  krebs @ apple.com |
| Re: |  |
| Abstract |  |
| Purpose | To propose resolution for MMS related comments for “P802.15.4ab™/D03 Draft Standard for Low-Rate Wireless Networks”. |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Sources” field above.It is offered as a basis for discussion and is not binding on the contributing individuals. The material in this document is subject to change in form and content after further study. The contributors reserve the right to add, amend or withdraw material contained herein. |

# CID 71 (Accepted)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Index #** | **Page** | **Sub-clause** | **Line #** | **Comment** | **Proposed Change** |
| 71 | 115 | 10.39.11.3.1 | 9 | "A Message Control field value of zero signals that the initiator supports Compact frames with Compact Frame ID field values of 0x01 to 0x06 with a Message Control field value of 0x00." "Message Control field value of 0x00" should be "Message ID field value of 0x00" | Change "… Message Control field value of 0x00" to "… Message ID field value of 0x00" |

Discussion: OK

Proposed resolution: Accepted.

Disposition detail: N/A