IEEE P802.19
Wireless Coexistence
Comment Resolution on CID#74	
Date:  2012-05-14	
Author(s):	
Name	Company	Address	Phone	Email	
Jinho Kim	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea	+82-31-450-1867	boiler4.kim@lge.com	
Jinyoung Chun	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea	+82-31-450-1856	jiny.chun@lge.com	
Suhwook Kim	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea			
Wookbong Lee	LGE				
Jinsam Kwak	LGE				
Abstract

This document provides normative text related to a the CID#74 for some editorial clarification of WSO deauthentication procedure.

	

CID	Clause	Subclause	Page	Line	Type	Comment	Suggested Remedy	Response	
74		5.2.1.2				In Fig. 9, "CM_Registration_Request" --> "CM_DeRegistration_Request" ?
Terminologically it looks confusing why a "CM_Registration_Request" need to be sent after "Deauthentication_Request" from CE to CM	TBD		

Discussion 
1.	As can be seen in the Fig. 9, CM_Registration_Request is described in the procedure of WSO deauthentication procedure.        Regardless whether the "Deauthencation_Request/response" initiate the "CM_Registration_Request" or not, it seems that two distintive procedures are dipicted in a procedure of deauthentication.     Thus, it looks confusing. 

 Proposed Text

-(Editor's note) In the Fig. 9, delete CDIS entity. If this explanation is really necessary, then mention the operation in a form of sentence in that section.   

5.2.1.2 WSO deauthentication procedure 
This procedure, illustrated in Figure 9, is performed when a CE receives a request to stop operation. 

Figure 9 ・WSO deauthentication procedure