IEEE P802.19  
Wireless Coexistence

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Updated description of the “Announcing available channel list change by WSO” procedure | | | | |
| Date: 2012-11-14 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Mika Kasslin | Nokia | Otaniementie 19, 02150 Espoo, Finland | +358-718036294 | mika.kasslin@nokia.com |
| Jari Junell | Nokia | Otaniementie 19, 02150 Espoo, Finland | +358-718036575 | jari.junell@nokia.com |

Abstract

This document contains proposed modifications to data type definitions in section 6.5 of the IEEE 802.19.1 draft DF3.02. Changes are highlighted with revision marks. Rationale for the changes is given in comment with CID87.

**Notice:** This document has been prepared to assist IEEE 802.19. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

* + - 1. Announcing available channel list change by WSO procedure

A CE shall perform the announcing available channel list change by WSO procedure to provide an updated list of available channels relevant to the WSO to the CM. An illustrative example of this procedure is shown in Figure 24. AvailableChannelsAnnouncement message is defined in clause 6.4.

Announcing_available_channel_list_change_by_device

1. — Announcing available channel list change by WSO procedure

A CE which has been previously requested by the CM to provide available channel list for the WSO which the CE represents shall generate an AvailableChannelsAnnouncement message when the available channel list has changed and send this AvailableChannelsAnnouncement message to the CM. CE operations related to generating and sending an AvailableChannelsAnnouncement message are specified in clause 7.

After the CM has received an AvailableChannelsAnnouncement message from the CE, the CM shall process the AvailableChannelsAnnouncement message. CM operations related to processing an AvailableChannelsAnnouncement message are specified in clause 8.