**IEEE P802.21  
Media Independent Handover Services**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Proposed Remedy for the 802.21c LB6b comment #144** | | | | |
| **Date:** 2013-06-08 | | | | |
| **Author(s):** | | | | |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Yoshihiro Ohba | Toshiba |  |  | yoshihiro.ohba@ toshiba.co.jp |

Abstract

This document contains proposed remedy for “the 802.21c ballot 6b comment #144 about PICS.

**Remedy for the 802.21c LB6b comment #144**

M.8 PICS proforma tables

**M.8.3 Major capabilities**

*Add the following rows into table in M.8.3 as shown:*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item number | Item description | References | Status | Support | Mnemonic |
| M.8.3.10 | Is optimized single-radio handover supported? | 5.2.3, 5.4.4, 5.5.8, 5.8, 5.9 | O | Yes [] No [] | MC10 |
| M.8.3.11 | Is key generation supported? | 9.2.2 | MC10.O | Yes [] No [] | MC11 |

*Add the following rows into table in M.8.3 as shown:*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| M.8.4.43 | MIH\_Prereg\_Xfer request | 8.6.3.24 | MC10.M | Yes [ ] No [ ] | PDU43 |
| M.8.4.44 | MIH\_Prereg\_Xfer response | 8.6.3.25 | MC10.M | Yes [ ] No [ ] | PDU44 |
| M.8.4.45 | MIH\_N2N\_Prereg\_Xfer request | 8.6.3.26 | MC10.M | Yes [ ] No [ ] | PDU45 |
| M.8.4.46 | MIH\_N2N\_Prereg\_Xfer response | 8.6.3.27 | MC10.M | Yes [ ] No [ ] | PDU46 |
| M.8.4.47 | MIH\_Prereg\_Ready request | 8.6.3.28 | MC10.M | Yes [ ] No [ ] | PDU47 |
| M.8.4.48 | MIH\_Prereg\_Ready response | 8.6.3.29 | MC10.M | Yes [ ] No [ ] | PDU48 |
| M.8.4.49 | MIH\_CTRL\_Transfer request | 8.6.3.30 | MC10.M | Yes [ ] No [ ] | PDU49 |
| M.8.4.50 | MIH\_CTRL\_Transfer response | 8.6.3.31 | MC10.M | Yes [ ] No [ ] | PDU50 |