**IEEE P802.21
Media Independent Handover Services**

|  |
| --- |
| **Proposed Remedy for the 802.21d LB7 comment #236**  |
| **Date:** 2013-08-26 |
| **Author(s):** |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Yoshihiro Ohba | Toshiba |  |  | yoshihiro.ohba@ toshiba.co.jp |

Abstract

This document contains proposed remedy for “the 802.21d ballot 7 comment #236 about PICS.

**Remedy for the 802.21c LB6b comment #236**

M.8 PICS proforma tables

**M.8.3 Major capabilities**

*Add the following rows into table in M.8.3 as shown:*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item number | Item description | References | Status | Support | Mnemonic |
| M.8.3.12 | Is multicast group management supported? | 8.4.2.3, 9.4 | O | Yes [] No [] | MC12 |

*(Note: Entries M.8.3.10 and M8.3.11 are defined in 802.21c.)*

*Add the following rows into table in M.8.4 as shown:*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| M.8.4.51 | MIH\_Configuration Update indication | 8.6.1.20 | MC12.M | Yes [ ] No [ ] | PDU51 |
| M.8.4.52 | MIH\_MN\_Group\_Manipulate request | 8.6.1.21 | MC12.M | Yes [ ] No [ ] | PDU52 |
| M.8.4.53 | MIH\_MN\_Group\_Manipulate response | 8.6.1.22 | MC12.M | Yes [ ] No [ ] | PDU53 |
| M.8.4.54 | MIH\_Net\_Group\_Manipulate request | 8.6.3.23 | MC12.M | Yes [ ] No [ ] | PDU54 |
| M.8.4.55 | MIH\_Net\_Group\_Manipulate indication | 8.6.3.24 | MC12.M | Yes [ ] No [ ] | PDU55 |
| M.8.4.56 | MIH\_Net\_Group\_Manipulate response | 8.6.3.25 | MC12.M | Yes [ ] No [ ] | PDU56 |
| M.8.4.57 | MIH\_Pull\_Credential request | 8.6.3.26 | MC12.M | Yes [ ] No [ ] | PDU57 |
| M.8.4.58 | MIH\_Pull\_Credential response | 8.6.3.27 | MC12.M | Yes [ ] No [ ] | PDU58 |
| M.8.4.59 | MIH\_Push\_Credential request | 8.6.3.28 | MC12.M | Yes [ ] No [ ] | PDU59 |
| M.8.4.60 | MIH\_Push\_Credential response | 8.6.3.29 | MC12.M | Yes [ ] No [ ] | PDU60 |
| M.8.4.61 | MIH\_Revoke\_Credential request | 8.6.3.30 | MC12.M | Yes [ ] No [ ] | PDU61 |
| M.8.4.62 | MIH\_Revoke Credential response | 8.6.3.31 | MC12.M | Yes [ ] No [ ] | PDU62 |

*(Note: Entries M.8.4.43 to M8.4.50 are defined in 802.21b and 802.21c.)*