IEEE P802.21.1  
Media Independent Services

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Remedy for Comment #160 of the WG LB9 on IEEE P802.21.1/D01 draft | | | | |
| Date: 2016-02-14 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Hyeong-Ho Lee | ETRI |  |  | [holee@etri.re.kr](mailto:holee@etri.re.kr) |

Abstract

This document contains proposed remedy for comment #160 of the WG LB9 on IEEE P802.21.1/D01 draft based on the LB9 comments file (DCN: 21-16-0008-05-SAUC).

**Proposed Remedy for Comment #160 of the WG LB9 on IEEE P802.21.1/D01 draft**

**Comment #160** (Annex H, Page 207, Line 6) PCS profoma tables for items specific to RRM and D2D are missing. Add PCS profoma tables for items specific to RRM and D2D.

* Response: We accept this comment, and agree to add PCS profoma tables for items specific to RRM and D2D.
* Remedy: Modify H.1 of Annex H as follows.

## PCS proforma tables

### Major capabilities

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item number**a | **Item description** | **References** | **Status** | **Support** | **Mnemonic** |
| H1.1.1 | Is Mobile Initiated Handover supported? | 5.7.2.3 | O.4 | Yes [ ] No [ ] | MC1 |
| H1.1.2 | Is Network Initiated Handover supported? | 5.7.2.4 | O.4 | Yes [ ] No [ ] | MC2 |
| H1.1.3 | Is optimized single-radio handover supported? | 5.3.2, 5.3.3, 5.4, 5.5 | O | Yes [ ] No [ ] | MC3 |
| H1.1.4 | Is MIS for SDRANs supported? | 6 | O | Yes [ ] No [ ] | MC4 |
| H1.1.5 | Is HEMS service supported? | 7 | O | Yes [ ] No [ ] | MC5 |
| H1.1.6 | Is RRM service supported? | 8 | O | Yes [ ] No [ ] | MC6 |
| H1.1.7 | Is D2D communication service supported? | 9 | O | Yes [ ] No [ ] | MC7 |

aFor all other items see IEEE Std 802.21-XXXX

### PDUs

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Item number**a | | **Item description** | | **References** | | **Status** | | **Support** | | **Mnemonic** | |
| H.1.2.1 | | MIS \_Link \_Handover \_Imminent indication? | | 5.13.2.1 | | MC1:O | | Yes [ ] No [ ] N/A[ ] | | PDU1 | |
| H.1.2.2 | | MIS\_Link\_Handover\_Complete indication? | | 5.13.2.2 | | MC1:O | | Yes [ ] No [ ] N/A[ ] | | PDU2 | |
| H.1.2.3 | | MIS\_Net\_HO\_Candidate\_Query  request? | | 5.13.3.1 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU3 | |
| H.1.2.4 | | MIS\_Net\_HO\_Candidate\_Query  response? | | 5.13.3.2 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU4 | |
| H.1.2.5 | | MIS\_MN\_HO\_Candidate\_Query  request? | | 5.13.3.3 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU5 | |
| H.1.2.6 | | MIS\_MN\_HO\_Candidate\_Query  response? | | 5.13.3.4 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU6 | |
| H.1.2.7 | | MIS\_N2N\_HO\_Query\_Resource  s request? | | 5.13.3.5 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU7 | |
| H.1.2.8 | | MIS\_N2N\_HO\_Query\_Resource  s response? | | 5.13.3.6 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU8 | |
| H.1.2.9 | | MIS\_MN\_HO\_Commit  request? | | 5.13.3.7 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU9 | |
| H.1.2.10 | | MIS\_MN\_HO\_Commit  response? | | 5.13.3.8 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU10 | |
| H.1.2.11 | | MIS\_Net\_HO\_Commit  request? | | 5.13.3.9 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU11 | |
| H.1.2.12 | | MIS\_Net\_HO\_Commit  response? | | 5.13.3.10 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU12 | |
| H.1.2.13 | | MIS\_Net\_HO\_Commit  indication? | | 5.13.3.11 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU13 | |
| H.1.2.14 | | MIS\_N2N\_HO\_Commit  request? | | 5.13.3.12 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU14 | |
| H.1.2.15 | | MIS\_N2N\_HO\_Commit  response? | | 5.13.3.13 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU15 | |
| H.1.2.16 | | MIS\_MN\_HO\_Complete  request? | | 5.13.3.14 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU16 | |
| H.1.2.17 | | MIS\_MN\_HO\_Complete  response? | | 5.13.3.15 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU17 | |
| H.1.2.18 | | MIS\_N2N\_HO\_Complete  request? | | 5.13.3.16 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU18 | |
| H.1.2.19 | | MIS\_N2N\_HO\_Complete  response? | | 5.13.3.17 | | MC2:M | | Yes [ ] No [ ] N/A[ ] | | PDU19 | |
| H.1.2.20 | | MIS\_Net\_HO\_Bcst\_Commit indication? | | 5.13.3.18 | | MC2:M | | Yes [ ] No [ ] N/A [ ] | | PDU20 | |
| H.1.2.21 | | MIS\_Prereg\_Xfer request | | 5.13.3.19 | | O | | Yes [ ] No [ ] | | PDU21 | |
| H.1.2.22 | | MIS\_Prereg\_Xfer response | | 5.13.3.20 | | O | | Yes [ ] No [ ] | | PDU22 | |
| H.1.2.23 | | MIS\_N2N\_Prereg\_Xfer request | | 5.13.3.21 | | O | | Yes [ ] No [ ] | | PDU23 | |
| H.1.2.24 | | MIS\_N2N\_Prereg\_Xfer response | | 5.13.3.22 | | O | | Yes [ ] No [ ] | | PDU24 | |
| H.1.2.25 | | MIS\_Prereg\_Ready request | | 5.13.3.23 | | O | | Yes [ ] No [ ] | | PDU25 | |
| H.1.2.26 | | MIS\_Prereg\_Ready response | | 5.13.3.24 | | O | | Yes [ ] No [ ] | | PDU26 | |
| H.1.2.27 | | MIS\_CTRL\_Transfer request | | 5.13.3.25 | | O | | Yes [ ] No [ ] | | PDU27 | |
| H.1.2.28 | | MIS\_CTRL\_Transfer response | | 5.13.3.26 | | O | | Yes [ ] No [ ] | | PDU28 | |
| H.1.2.29 | | MIS\_Resource\_Allocation request | | 8.5.1.1 | | O | | Yes [ ] No [ ] | | PDU29 | |
| H.1.2.30 | | MIS\_Resource\_Allocation response | | 8.5.1.2 | | O | | Yes [ ] No [ ] | | PDU30 | |
| H.1.2.31 | | MIS\_Resource\_Report request | | 8.5.2.1 | | O | | Yes [ ] No [ ] | | PDU31 | |
| H.1.2.32 | | MIS\_Resource\_Report response | | 8.5.2.2 | | O | | Yes [ ] No [ ] | | PDU32 | |
| H.1.2.33 | | MIS\_Link\_Preparation request | | 8.5.3.1 | | O | | Yes [ ] No [ ] | | PDU33 | |
| H.1.2.34 | | MIS\_Link\_Preparation response | | 8.5.3.2 | | O | | Yes [ ] No [ ] | | PDU34 | |
| H.1.2.35 | | MIS\_D2D\_Connection request | | 9.4.2.1 | | O | | Yes [ ] No [ ] | | PDU35 | |
| H.1.2.36 | | MIS\_D2D\_Connection response | | 9.4.2.2 | | O | | Yes [ ] No [ ] | | PDU36 | |

aFor all other items see IEEE Std 802.21-XXXX